The instructions for T5&T5e firmware upgrade.

1. Please format your micro SD card. Store the firmware to the root directory of your SD card (Don't change the file name or anything).

2. Connect the camera (with SD card) with the power socket (NOT Computer) or make sure the battery have the enough power and turn it on.

3. Find the version number in the setting last one,click the OK (wifi)button,and then choose to FW update.

4. Wait until the blue lights are off, it will turn on automatically,and then power on again, it need about 2mins.

